Pin Configuration of back charging port

Orientation of pins with charging ports facing upwards.

|  |  |  |  |
| --- | --- | --- | --- |
| M | M | B | T |

M= middle

B= bottom

T= top

To charge the top battery:

Orange lead -> T

White lead -> Either M

To charge bottom battery

Orange lead -> Either M

White lead -> B

The red light will be on the power converter as long as it has power.

The green light will be on while the battery is charging. Once the battery is fully charged, the green light will go off.